{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet2"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet2","index":0,"n_rows":45,"n_cols":7,"rows_kept":45,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,5],[2,6,2,11],[3,0,3,5],[23,1,23,4],[24,1,24,5],[39,1,39,4],[40,1,40,5],[44,1,44,4]],"flags":["formulas_cached_only"]}
["民用航空器火灾科学重点实验室办公楼维修工程改装清单"]
["                                                                             基  础  装  修"]
["工程地址：广汉",{"$nulls":5},"工程总造价："]
["客户姓名：",{"$nulls":5},"客户联系方式："]
["序号","项目名称","单位","工程量","单价","合价","材料及施工工艺说明"]
[1,"地面地坪漆","m2",768,null,null,"打磨底涂+刮灰中涂+面漆涂（共刷三遍，2mm厚，灰色地坪漆）"]
[2,"门拆除","樘",35,null,null,"人工+机械损耗"]
[3,"正门玻璃门","m2",18.2,null,null,"正门玻璃门（10mm钢化玻璃，30边框），两樘"]
[4,"侧门2封门洞","m2",4.2,null,null,"木工板+水泥板，刮白，乳胶漆饰面"]
[5,"防盗门","樘",32,null,null,"型号：甲级门，9cm门扇，2mm门框厚度，7cm门边框。品牌：成都米悦钢质门"]
[6,"入户梯步贴砖","m2",26,null,null,"水泥(绵竹蓝绵水泥）+中沙+人工费（含机具损耗）；水泥砂浆厚度30mm以内，"]
[7,"入户梯步砖","m2",26,null,null,"800*800米白色玻化砖，拉槽"]
[8,"墙砖拆除","m2",70,null,null,"人工+机械损耗"]
[9,"砖拆除","项",1,null,null,"两个卫生间洗漱台和隔墙拆除，人工+机械损耗"]
[10,"卫生间贴砖","m2",69,null,null,"水泥(绵竹蓝绵水泥）+中沙+人工费（含机具损耗）；水泥砂浆厚度30mm以内，"]
[11,"卫生间砖","m2",69,null,null,"地砖：300*300/墙砖：300*600。广东砖"]
[12,"蹲便+水箱","套",6,null,null,"含安装"]
[13,"洗手台石材台面","个",2,null,null,"黑色大理石台面+陶瓷洗手盆+龙头"]
[14,"拖布池","个",2,null,null,"成品拖布池，含安装"]
[15,"蹲位隔断","个",6,null,null,"颗粒防潮板+五金，灰色（人工+材料）"]
[16,"蹲位抬高","m2",6,null,null,"人工，水泥，红砖"]
[17,"新建120墙","m2",8.6,null,null,"标砖红砖（称重需要得部分）+加气砖砖混合砌筑（不承重活不开孔部分）+双面抹灰+人工+水泥砂浆"]
[18,"新建120砖墙双面抹灰","m2",17.2,null,null,"人工，水泥"]
[null,"小计",{"$nulls":4},0]
[null,"水电工程"]
[1,"led灯","套",32,null,null,"室内照明，日光灯管(飞利浦）"]
[2,"配电箱","套","1",null,null,"空调用电控制"]
[3,"空调插座","个",29,null,null,"室内空调（飞雕）"]
[4,"过道吸顶灯（声控）","个",14,null,null,"公共区域照明"]
[5,"水管材料（给排水）","项",1,null,null,"卫生间改造，ppR管管件，pvc一U排水管管件"]
[6,"人工费","项",1,null,null,"插座，灯具，桥架，给排水安装，电缆布放，草坪开挖及恢复，配电箱安装"]
[7,"配电箱","套","6",null,null,"实验室动力用电配电箱"]
[8,"配电柜","套",1,null,null,"由户外配电柜引入本楼层主配电柜"]
[9,"120mm带铠电缆","m",90,null,null,"185mm电缆线"]
[10,"10mm平普通电缆","m",120,null,null,"实验室动力用电"]
[11,"6mm平线改造","m",2000,null,null,"空调用电"]
[12,"辅料","项",1,null,null,"穿线管等材料"]
[13,"电力桥架（300*200）","m",90,null,null,"电览电线"]
[14,"开空调孔+穿墙孔","个",58,null,null,"人工+机械损耗"]
[null,"小计",{"$nulls":4},0]
[null,"其他项目"]
[1,"材料运输及搬运",{"$nulls":4},"装修材料的运输及搬运费用(只含装饰公司的材料)。"]
[2,"日常保洁",{"$nulls":4},"日常清洁及完工保洁。"]
[3,"建渣清运+外运",{"$nulls":4},"清理至符合垃圾处理场所"]
[null,"小计"]